{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["明细表"],"not_rendered":{"images":7,"external_links":2,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"明细表","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"merged":[[0,0,0,6],[12,1,12,6]],"flags":["formulas_cached_only"]}
["附件1：VI系统导视指示牌制作要求"]
["序号","项目内容","材质/工艺/规格尺寸/型号/安装","规格","数量","单位","备注"]
[1,"楼梯楼层标识牌","整体框架采用304 1.2厚镜面不锈钢板激光切割板形，烤漆镂空,刨坑压折箱体 焊接，内置30*30镀锌钢方管结构焊接， 打磨抛光 电镀玫瑰金色，图文蚀刻填色或金属字。面板+亚克力+LED灯","1.6X0.585",52,"个"]
[2,"楼层布局图总指引标识牌","整体框架采用304 1.2厚镜面不锈钢板激光切割板形，烤漆镂空,刨坑压折箱体 焊接，内置30*30镀锌钢方管结构焊接， 打磨抛光 电镀玫瑰金色，图文蚀刻填色或金属字。面板+亚克力+LED灯","1.6X1.36X0.1",22,"个"]
[3,"门牌标识","整体框架采用304 1.2厚镜面不锈钢板激光切割板形，烤漆镂空,刨坑压折箱体 焊接， 打磨抛光 电镀玫瑰金色，图文蚀刻填色或金属字。面板尺寸","0.3x0.12x0.31",412,"个"]
[4,"电梯楼层指引标识牌","整体框架采用304 1.2厚镜面不锈钢板激光切割板形，烤漆镂空,刨坑压折箱体 焊接，内置30*30镀锌钢方管结构焊接， 打磨抛光 电镀玫瑰金色，图文蚀刻填色或金属字。面板+亚克力+LED灯","0.82x0.3x1",51,"个"]
[5,"区域禁止提示牌","整体框架采用304 1.2厚镜面不锈钢板激光切割板形，烤漆镂空,刨坑压折箱体 焊接，打磨抛光 电镀玫瑰金色，图文蚀刻填色或金属字。面板尺寸，标准规格8个一组计算。","0.3x0.12x0.1",98,"组"]
[6,"区域竖式标识牌","整体框架采用304 1.2厚镜面不锈钢板激光切割板形，烤漆镂空,刨坑压折箱体 焊接，内置30*30镀锌钢方管结构焊接， 打磨抛光 电镀玫瑰金色，图文蚀刻填色或金属字。面板+亚克力+LED灯","0.4x1.1",149,"个"]
[7,"区域方向指示牌","整体框架采用304 1.2厚镜面不锈钢板激光切割板形，烤漆镂空,刨坑压折箱体 焊接，内置30*30镀锌钢方管结构焊接， 打磨抛光 电镀玫瑰金色，图文蚀刻填色或金属字。面板+亚克力+LED灯","2.395x0.38",63,"个"]
[8,"强弱电井、机房，工程标识等","采用PVC亚克力","0.21X0.1",200,"个"]
[9,"本次项目安装费用","项目内安装人工和材料费用",null,30,"天","整体制作安装工期30天"]
[10,"本次项目物料运输费用","所有运费"]
[null,"备注                                                                                                                                            制作材料：通常选用不锈钢镜面或拉丝板，钛金板，玻璃，亚克力板，铜板，铝板，冷轧板，不锈钢管，实木作为表面材料，内部结构采用不锈钢管，黑色金属型材为加强材料，发光源用led,等离子灯，导光板等相关材料。\n制作工艺：金属采用焊接，折弯，洗槽，车床，水切割，线切割，打磨，抛光，拉丝，电镀，氧化，腐浊，烤漆。亚克力和玻璃表面采用丝印，贴即时贴，雕刻，喷砂等工艺根据设计图纸来综合加工。标识的完美关键在设计理念和制作工艺的合理性。\n"]