{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["清单"],"not_rendered":{"defined_names":552},"read":"whole","date_system":"1900"}

{"sheet":"清单","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"merged":[[0,0,0,9],[1,0,4,2],[1,3,2,9],[3,3,3,9],[4,3,4,9],[5,0,5,9],[22,0,22,9],[31,0,31,9],[37,1,38,1],[41,0,41,9],[51,1,52,1],[51,2,52,2],[53,1,54,1],[53,2,54,2],[58,0,58,9]]}
["花都区颐养院2号楼4至8层视频监控系统、无线wifi系统及视频解码大屏升级改造项目配置清单"]
["建设需求：",null,null,"一、2号楼新增部分（4一8层共增加36个摄像点）\n1、四层通道公共区域新增4个摄像点位，2个楼梯口区域新增2个摄像点位（共6个摄像点位）；\n2、五层通道公共区域新增4个摄像点位，2个楼梯口区域新增2个摄像点位（共6个摄像点位）；\n3、六层通道公共区域新增4个摄像点位，2个楼梯口区域新增2个摄像点位（共6个摄像点位）；\n4、七层通道公共区域新增5个摄像点位，2楼梯口区域新增2个摄像点位，平台公共区域新增4个摄像点位（共11个摄像点位）；\n5、八层通道公共区域新增5个摄像点位，2楼梯口区域新增2个摄像点位(共7个摄像点位）；\n"]
[]
[{"$nulls":3},"二、2号楼新增部分（4一8层共增加29个无线WIFI）\n1、四层通道公共区域新增6个无线WIFI点，连廊区域新增1个无线WIFI点（共7个无线WIFI点）；\n2、五层通道公共区域新增6个无线WIFI点，连廊区域新增1个无线WIFI点（共7个无线WIFI点）；\n3、六层通道公共区域新增6个无线WIFI点，连廊区域新增1个无线WIFI点（共7个无线WIFI点）；\n4、七层通道公共区域新增4个无线WIFI点（共4个无线WIFI点）；\n5、八层通道公共区域新增4个无线WIFI点(共4个无线WIFI点）；"]
[{"$nulls":3},"三、监控中心建设3*2拼接大屏（共6块大屏，尺寸：3200*2800*650）"]
["1、监控中心部分"]
["序号","设备名称","品牌","产品型号","产品参数","购买数量","单位","备注"]
[1,"安防综合平台管理一体机","海康威视","iVMS-9000N-S5 V2.0","2U标准机架式5盘位双板通用安防一体机，ATX电源\n64位多核高性能处理器\nDDR4高频率内存条\n1个HDMI接口、1个DP接口\n2个10M/100M/1000Mbps网口\n2个USB2.0接口、2个USB3.0接口",1,"台"]
[2,"视频解码器","海康威视","DS-6A10UD","HDMI接口输出265解码板（不支持MPEG-2）持4路HDMI信号输出，支持解码2路2400W@25fps、或4路1200W@25fps、或8路800W@25fps、或16路400W@25fps、或 32路200W@25fps，或64路720P@25fps及以下分辨率（例如4CIF）。奇数口支持3840x2160@30Hz及以下标准分辨率输出，偶数口支持1080p及以下标准分辨率输出",1,"台"]
[3,"55寸超窄边液晶拼接单元","PFT","PFT-F55","55寸超窄边拼接单元，物理拼缝：1.7mm,对比度4000:1,50000小时超长寿命,物理分辨率1920*1080，亮度500cd/m2，响应时间8ms。支持输入VGA、Video、DVI、HDMI，RJ45接口控制，单元含内置图像处理器，自由无限拼接功能。",6,"台"]
[4,"大屏线缆及配件","定制","定制","每套屏幕对应的HDMI线、电源、显示和控制线缆及接口等配件",6,"套"]
[5,"安装支架系统","定制","--","专用安装支架",6,"套"]
[6,"存储录像机","海康","DS-8864N-R16","16盘位 400M支持视频流和图片、视频文件进行混合直写存储；2U机架式，单控制器、冗余电源、支持SATA硬盘；64位多核处理器，4GB高速缓存",1,"台","用于2号监控点"]
[7,"监控级硬盘","西数","8TB","监控级硬盘8TB",8,"块","存储60天"]
[8,"核心交换机","锐捷","RG-NBS5710-24GT4SFP-E","24个10/100/1000M自适应电口，4个SFP光口                                                           交换容量：336Gbps/3.36Tbps  包转发率：51Mpps/126Mpps",1,"台"]
[9,"汇聚核心交换机","锐捷","RG-NBS5100-24GT4SFP","三层网管交换机，交换容量336Gbps，包转发率42Mpps，24口10/100/1000Mbps自适应电口交换机，固化4个SFP千兆光口，支持VLAN、ACL、端口镜像、端口聚合",1,"个","用于2号楼汇聚于监控中心"]
[10,"HDMI线","绿联",null,"20米，专业视频线",1,"条","用于联接原有大屏分配器"]
[11,"理线架","国标","－","1U高度，支持标准机柜安装",3,"个"]
[12,"42网络机柜","图腾",6642,"机柜尺寸：800宽*1200深*2000高",1,"台"]
[13,"机柜电源PDU插座","为安","八位防雷PDU","Un=220V，额定=10A，  标称放电5kA      最大放电10kA",3,"个"]
[14,"中心机房设备安装、调试","定制","－","安装、标识、整理、调试",1,"项"]
[15,"平台整体调试服务费","定制","－","安装、调试、维护",1,"项"]
["2、2号楼监控前端设备部分"]
["序号","设备名称","品牌","产品型号","产品参数","购买数量","单位","备注"]
[1,"半球型摄像机\n(400W全彩)","海康","DS-2CDB145","400万全彩1/2.7”CMOS 半球型网络摄像机\n最小照度:彩色: 0.005 Lux @(F1.2,AGC ON), 0 Lux with IR",36,"个"]
[2,"摄像机支架","海康","－",null,36,"个","摄像机尾端使用"]
[3,"收线盒","定制","－",null,36,"个","摄像机尾端使用"]
[4,"千兆POE交换机","海康","DS－3E0508E","8口千兆，2口FFT 高工功率230W",10,"个","安装楼层点汇聚"]
[5,"网络收发器","锐捷","RC－YS110","千兆1光1电",5,"对","用于中心传传输"]
[6,"分端机柜","图腾","9U","加厚型，540*600*450",5,"个","安装于楼层弱电井间"]
[7,"摄像机辅材","定制",null,"接线端、水晶头等",36,"套","用于安装各摄像机"]
["3、2号楼无线WIFI部分"]
["序号","设备名称","品牌","产品型号","产品参数","购买数量","单位","备注"]
[1,"AP管理器","华为","AirEngine 9700S-S","1. 无线标准\n支持Wi-Fi 6（802.11ax），向下兼容802.11a/b/g/n/ac。\n2. 频段\n双频并发：2.4 GHz和5 GHz。\n3. 无线速率\n整机速率可达5.95 Gbps。\n2.4 GHz频段速率：573.5 Mbps。\n5 GHz频段速率：4.8 Gbps。",1,"台","用于网络中心"]
[2,"AC软件授权","华为","L-WAC-S－1AP","授权许可",50,"套"]
[3,"核芯交换机","华为","S5735S-S24T4X","三层交换机核辛交换机，24个10/100/1000BASE-T以太网端口，4个万兆SFP+、‌\n端口配置‌: 24个10/100/1000Base-T电口 + 4个万兆SFP+光口\n‌转发性能‌: 96Mpps\n‌交换容量‌: 336Gbps",1,"台","策划三层核芯"]
[4,"高密度无线AP","华为","AirEngine 5762S","无线性能‌\n‌无线标准‌: Wi-Fi 6（802.11ax）\n‌频段与速率‌:\n‌2.4GHz‌: 4×4 MIMO，最高 574Mbps\n‌5GHz‌: 4×4 MIMO，最高 2.4Gbps\n‌整机速率‌: 约 ‌3Gbps‌\n‌最大用户数‌: 支持 ‌256‌ 终端并发接入\n‌关键技术‌: OFDMA、MU-MIMO、智能射频调优",29,"个","用于2号楼各层区域"]
[5,"汇聚POE交换机","华为","S1730S-L8P4S－A","8×10/100/1000Base-T PoE+电口 + 2×千兆SFP上行光口\n单端口最大30W，整机最大240W（支持802.3af/at标准）",6,"个","楼层汇聚"]
[6,null,"华为","S1730S-L16P2SR","16×10/100/1000Base-T PoE+电口 + 2×千兆SFP上行光口\n单端口最大30W，整机最大240W（支持802.3af/at标准）",2,"个","楼层汇聚"]
[7,"网络收发器","锐捷","RC－YS110","千兆1光1电",5,"对","用于网络物理格理"]
[8,"安装辅材","定制",null,"吊顶支架、水晶头等",29,"套","用于安装设备"]
["4、安装配件及安装人工"]
["序号","设备名称","品牌","产品型号","产品参数","购买数量","单位","备注"]
[1,"网线","海康",null,"国标纯铜网线",3850,"米","部分线路利旧"]
[2,"光纤","联讯","单模","单横 4芯",500,"米","用于各楼层汇聚"]
[3,"光纤","联讯","单模","单横 8芯",550,"米","与综合楼监控中心汇聚"]
[4,"光纤跳线","联讯",null,"跳线FC",60,"条"]
[5,"光纤尾纤","联讯",null,"尾纤FC",60,"条"]
[6,"光端盒","联讯",null,"FC 4口",16,"个"]
[7,"72芯ODF架","联讯",null,"72芯电信级满配",1,"套"]
[8,"光纤熔接","定制",null,"端测国标",90,"芯"]
[9,"电源线","科宇达",null,"RVV3*2.5",660,"米","主干设备供电"]
[10,{"$nulls":3},"RVV3*1.5",200,"米","分支设备供电"]
[11,"PVC线管","国产",null,"PVC20",800,"米"]
[12,{"$nulls":3},"PVC25",600,"米"]
[13,"PVC波纹管","国产",null,25,4,"卷"]
[14,"辅材","定制",null,"线管、线槽及安装辅材",1,"批"]
[15,"安装人工费","定制",null,"暗装线路、铺设安装、检测、调试、维护",70,"工","含干汇聚线路"]
["注：报价含运输费、安装费、税票，含维护1年。"]